# Cable Requirements

Your KX3 must be connected to a personal computer serial COM port before firmware can be sent.

## KXUSB interface cable for USB

A KXUSB interface cable for USB plugs into a USB port on your personal computer. Insert the right-angled 3.5 mm plug into your KX3's ACC1 jack.

## KXSER RS-232 interface cable

A KXSER RS-232 interface cable plugs into an RS-232 serial port or a USB to Serial adapter, such as the Elecraft KUSB USB to Serial Adapter. Insert the 3.5 mm plug into your KX3's ACC1 jack.